{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["問題","実習","解答"],"not_rendered":{"charts":2,"images":2,"macros":1,"external_links":0,"defined_names":8,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"問題","index":0,"n_rows":3,"n_cols":2,"rows_kept":3,"cut":false,"hidden":false,"merged":[[1,1,1,8],[2,1,35,8]]}
[]
[null,"問題10.1 原発汚染水からのセシウム連続吸着操作 [ゴールシーク]"]
[null,"　放射性物質であるセシウムを含む排水（セシウム濃度CF=0.000015 mol L-1、流量Q=5 L min-1）を、完全混合（吸着装置内の濃度が均一であり、装置出口の濃度に等しい）の吸着装置で連続的に吸着処理を行う。吸着剤であるゼオライト（モラキュラーシーブ：粘土鉱物の一種で、規則的なチャンネル（管状細孔）とキャビティ（空洞）を有する剛直な陰イオン性の骨格からなるアルカリまたはアルカリ土類金属を含む含水アルミノケイ酸塩）は、S=20 g min-1の流量で装置に流入出する。吸着平衡（平衡吸着量q [mol-セシウム (g-ゼオライト)-1]と残留吸着物質濃度Cの関係）はフロインドリッヒ式で表される。\n        \n　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　 (10.1)\n\n　等温吸着実験から、フロインドリッヒ式のパラメータは , k=5.82×10-4 [mol1-1/n (g L-1/n)-1]、n=2.37と求められている。セシウム吸着における物質移動容量係数はkLa=0.0015 min-1である。図10.2に示す連続吸着操作において，滞留時間tres（汚染水が吸着装置内に留まる時間。吸着塔体積Vを汚染水の体積流速Qで除して求める）と出口におけるセシウム濃度Coutの関係を、滞留時間tresを120 min間隔で1200 minまで変化させた場合について求めなさい。\n\n\n\n\n\n\n\n\n\n\n\n　　　　　　　　　　　　図10.2 連続吸着装置におけるセシウムの除去"]

{"sheet":"実習","index":1,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,0,1,1],[6,0,6,1]]}
[]
["物質移動係数、吸着式パラメーター"]
["物質移動容量係数　kLa　[min-1]",1.5E-3]
["フロインドリッヒ式パラメーター　k [mol1-1/n (g L-1/n)-1]",5.8200000000000005E-4]
["フロインドリッヒ式パラメーター n [-]",2.37,null,"排水"]
[null,null,null,"Q [L min-1]",5,null,null,null,null,"処理水"]
["吸着装置の運転条件",null,null,"CF [mol L-1]",1.5E-5,null,null,null,"Cout [mol L-1]",null,"?"]
["排水の流量 Q [L min-1]",5]
["排水中のセシウム濃度 CF [mol L-1]",1.5E-5]
["ゼオライトの流量　S [g min-1]",20]
[null,null,null,"吸着剤"]
[null,null,null,"S [g min-1]",20,null,null,null,"qout [mol g-1]",{"$f":"(E7-J7)*E6/E12","v":3.7500000000000005E-6}]
[]
[]
[]
[]
[null,null,"tres [min]","Cout [mol L-1]","残余関数の値"]

{"sheet":"解答","index":2,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[[1,0,1,1],[6,0,6,1]]}
[]
["物質移動係数、吸着式パラメーター"]
["物質移動容量係数　kLa　[min-1]",1.5E-3]
["フロインドリッヒ式パラメーター　k [mol1-1/n (g L-1/n)-1]",5.8200000000000005E-4]
["フロインドリッヒ式パラメーター n [-]",2.37,null,"排水"]
[null,null,null,"Q [L min-1]",5,null,null,null,null,"処理水"]
["吸着装置の運転条件",null,null,"CF [mol L-1]",1.5E-5,null,null,null,"Cout [mol L-1]",null,"?"]
["排水の流量 Q [L min-1]",5]
["排水中のセシウム濃度 CF [mol L-1]",1.5E-5]
["ゼオライトの流量　S [g min-1]",20]
[null,null,null,"吸着剤"]
[null,null,null,"S [g min-1]",20,null,null,null,"qout [mol g-1]",{"$f":"(E7-J7)*E6/E12","v":3.7500000000000005E-6}]
[]
[]
[]
[]
[null,null,"tres [min]","Cout [mol L-1]","残余関数の値"]
[null,null,0,1.5E-5,{"$f":"D18-($B$9+$B$3*C18*(($B$9-D18)/($B$10/$B$8*$B$4))^$B$5)/(1+$B$3*C18)","v":0}]
[null,null,120,1.2693049762303089E-5,{"$f":"D19-($B$9+$B$3*C19*(($B$9-D19)/($B$10/$B$8*$B$4))^$B$5)/(1+$B$3*C19)","v":-3.0403523835226078E-8}]
[null,null,240,1.1021642052877151E-5,-8.0936177539950242E-8]
[null,null,360,9.8337012545419521E-6,-8.6594271611463997E-8]
[null,null,480,8.9579748943316009E-6,-7.4454571424629838E-8]
[null,null,600,8.2900930605078406E-6,-5.6559402226878119E-8]
[null,null,720,7.7646579168537167E-6,-3.9162854429734243E-8]
[null,null,840,7.3373610572160314E-6,-2.8407092737339971E-8]
[null,null,960,6.9895558386126251E-6,-1.4804263647594969E-8]
[null,null,1080,6.6976001518401824E-6,-4.7755032015482204E-9]
[null,null,1200,6.3885587010485326E-6,-7.646888105074671E-8]