{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["問題","実習","解答"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":80,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"問題","index":0,"n_rows":3,"n_cols":2,"rows_kept":3,"cut":false,"hidden":false,"merged":[[1,1,1,8],[2,1,10,8]]}
[]
[null,"問題3.1 フォトフェントン反応による農薬分解 [VBA、シンプソン則：数値積分]"]
[null,"　フォトフェントン反応により農薬を分解する回分操作の反応装置を設計する。ラボ実験の結果より，フォトフェントン反応による農薬の分解を擬1次反応（分解は1次反応として表せるが，反応速度定数が農薬の初期濃度やそのほかの反応条件で変わるような反応）と近似した場合の擬1次反応速度定数kは0.1 min-1であった。設計する反応装置による農薬を含む排水の処理量Qは298 m3 day-1であり，初期農薬濃度C0は100 mg L-1である。処理後の農薬濃度Cを0.1 mg L-1以下にしたい場合に必要な反応装置の体積V [m3]を求めなさい。"]

{"sheet":"実習","index":1,"n_rows":6,"n_cols":4,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
[]
[null,"擬1次反応速度定数","k [min-1]",0.1]
[null,"初期農薬濃度","C0 [mg L-1]",100]
[null,"処理後農薬濃度","C [mg L-1]",0.1]
[null,"排水流量","Q [m3 day-1]",298]
[null,"反応槽の容積","V [m3]"]

{"sheet":"解答","index":2,"n_rows":6,"n_cols":4,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
[]
[null,"擬1次反応速度定数","k [min-1]",0.1]
[null,"初期農薬濃度","C0 [mg L-1]",100]
[null,"処理後農薬濃度","C [mg L-1]",0.1]
[null,"排水流量","Q [m3 day-1]",298]
[null,"反応槽の容積","V [m3]",14.321696101036347]