{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["問題","実習&解答"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"問題","index":0,"n_rows":3,"n_cols":2,"rows_kept":3,"cut":false,"hidden":false,"merged":[[1,1,1,8],[2,1,6,8]]}
[]
[null,"問題6.3 バイオフィルター出口における悪臭物質の濃度\n[VBA：ニュートン－ラフソン法]"]
[null,"　問題6.2では式(6.12)を、ゴールシークを用いて解くことでバイオフィルター内の濃度分布を求めた。ここではバイオフィルターの出口(z=L=0.9m)の濃度Cを、ゴールシークではなく、VBAによるニュートン-ラフソン法を使って求めなさい。\n"]

{"sheet":"実習&解答","index":1,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[[9,1,9,4],[9,5,9,7],[0,1,0,2]]}
[null,"データ"]
[null,"mm' [g m-3 hr-1]",380]
[null,"Ks' [g m-3]",5.0999999999999996]
[null,"m [-]",0.8]
[null,"Cin [g m-3]",10.5]
[null,"A [m2]",8.6E-3]
[null,"L [m]",0.9]
[null,"Q [m3 hr-1]",0.21]
[]
[null,"cal.",null,null,null,"収束過程の出力"]
[null,"z [m]","C [g m-3]","残余関数","収束計算回数","C [g m-3]","残余関数","収束計算回数"]
["出口",0.9]